{"text_format":"1","workbook":"xlsx","n_sheets":22,"sheets":["Cover Page","Contents","Facility Info","Operational Data","Operational Summary","Perf. Form 1","Energy Form 1","Permit Compliance","Improvements","Public Liasion","CO2 N2O","Residue Quality ","Water","Air (periodic)","Air (CEMS)","HCl","SO2","NOx","TOC","Particulates","CO 95% 10 min","NH3"],"not_rendered":{"charts":7,"images":2,"macros":1,"external_links":0,"defined_names":22,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover Page","index":0,"n_rows":53,"n_cols":14,"rows_kept":53,"cut":false,"hidden":false,"merged":[[13,13,18,15],[34,1,34,8],[0,3,5,6],[7,1,23,8],[28,1,28,8],[30,1,30,8],[32,1,32,8],[48,2,48,3],[48,6,48,8],[52,2,52,3],[36,1,36,8],[40,2,40,8],[42,2,42,4],[44,2,44,4],[46,2,46,3],[46,6,46,8]]}
[null,null,null,"Add company logo"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Version 22.3  30/11/22"]
[]
[]
[]
[]
[]
[null,"Add photo"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"This template may require adjustments by individual operators to meet specific reporting requirements as defined in the site Permit(s)"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"Annual Performance Report 2023"]
[]
[null,"Permit EPR/HP3247QS"]
[]
[null,"Dudley Energy from Waste"]
[]
[null,"other name of facility (if applicable)"]
[]
[null,"Urbaser Environmental Ltd"]
[]
[null,"Year:",2023]
[]
[null,"Address:","Lister Road, Dudley, DY2 8YT"]
[]
[null,"Tel: ","01384 900729"]
[]
[null,"Email: ","cpearce@urbaser.co.ik"]
[]
[null,"Prepared by:","Carl Pearce",null,null,"Position:","QHSE Advisor"]
[]
[null,"Approved by:","Jacob Towl",null,null,"Position:","Environmental Technician"]
[]
[null,"Version:",1]
[]
[null,"Issue Date:","2024-01-24"]

{"sheet":"Contents","index":1,"n_rows":45,"n_cols":11,"rows_kept":45,"cut":false,"hidden":false,"merged":[[4,10,7,14],[8,1,8,6],[3,1,3,6],[4,1,4,6],[5,1,5,6],[6,1,6,6],[7,1,7,6],[21,1,21,6],[9,1,9,6],[10,1,10,6],[11,1,11,6],[13,1,13,6],[14,1,14,6],[15,1,15,6],[16,1,16,6],[17,1,17,6],[18,1,18,6],[19,1,19,6],[20,1,20,6],[12,1,12,6],[36,1,36,6],[22,1,22,6],[23,1,23,6],[24,1,24,6],[27,1,27,6],[28,1,28,6],[29,1,29,6],[30,1,30,6],[31,1,31,6],[32,1,32,6],[35,1,35,6],[44,0,47,9],[37,1,37,6],[38,1,38,6],[39,1,39,6],[40,1,40,6],[41,1,41,6],[42,1,42,6]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Contents",null,null,null,null,null,null,null,null,null,"Notes:"]
["Section","Subject",null,null,null,null,null,"Page ",null,null,"Section references and Page nos. to be inserted"]
[null,"Facility Information",null,null,null,null,null,null,null,null,"Sections and Subjects may require adjustment by individual operators to meet specific reporting requirements as defined in the sites Permit(s)"]
[null,"Operational Data"]
[null,"Operational Summary"]
[null,"Performance Form 1"]
[null,"Energy Form 1"]
[null,"Permit Compliance"]
[null,"Improvements"]
[null,"Public Liasion"]
[null,"Carbon dioxide and nitrous oxide emissions"]
[null,"Residue Quality "]
[null,"Emissions to Water"]
[null,"Emissions to Air (periodically monitored)"]
[null,"Emissions to Air (continuously monitored)"]
[null,"Hydrogen Chloride emissions"]
[null,"Sulphur Dioxdie emsissions"]
[null,"Oxides of Notrigen emissions"]
[null,"Total Organic Carbon emissions"]
[null,"Particulate Matter emissions"]
[null,"Carbon Monoxide emissions"]
[null,"Ammonia emissions"]
[]
[]
["Version Control"]
["Section","Information",null,null,null,null,null,"Date"]
[]
[]
[]
[]
[]
[]
["Distribution"]
["Copy","Name, Role",null,null,null,null,null,"No."]
[]
[]
[]
[]
[]
[]
[]
[]
["This report is required under the Industrial Emissions Directive’s Article 55(2) requirements on reporting and public information on waste incineration plants and co-incineration plants, which require the operator to produce an annual report on the functioning and monitoring of the plant and make it available to the public. "]

{"sheet":"Facility Info","index":2,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[[4,0,17,8],[21,0,53,8],[4,10,13,13],[21,10,30,13]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Plant Description and Design",null,null,null,null,null,null,null,null,null,"Notes:"]
[]
["The main purpose of the activity at the installation is to burn municipal waste and to recover energy in the \nform of steam and electricity for export to the local grid. The installation includes waste receipt and storage, \nthe waste heat boilers, the abatement of the exhaust gas, the on-site storage of residues and all systems for \ncontrolling and monitoring incinerator operation. The plant is designed to process approximately 105,000 \ntonnes of waste per annum/12 tonnes per hour in two combustion streams. The heat produced is used to \ngenerate 7.145 MW of electricity.",null,null,null,null,null,null,null,null,null,"Include summary of plant design, design capacity, no. of combustion lines, electrical and heat capacity and any other general information that descibes the facility, its location and purpose "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Summary of Operational Processes and Procedures"]
[]
["The material is loaded into each of the furnaces via feed hoppers from a reception hall, where the waste \nvehicles deposit their loads into the storage bunkers. After entering the combustion chamber via the refuse \nfeed ram the material is allowed to fall onto the grate in a controlled manner. The moving grate mechanisms \nare used to agitate the waste as it progresses down to the ash discharge. As the waste moves along, \nprimary air is introduced from beneath the grate causing the waste to go through a series of drying and \nburning areas. Secondary air is introduced from above the grate for combustion control. Auxiliary oil fired \nburners are located in the combustion chambers both to heat it up on start up and to maintain the final gas \ntemperature. The hot gases are maintained at a minimum temperature of 850°C for 2 seconds in the \ncombustion chamber before passing to the boiler, economiser and abatement plant. Each furnace is \nequipped with a 2-pass water tube boiler raising steam at 45 bar and 355°C. Economisers are fitted down \nstream of each boiler unit to pre-heat the incoming feed water. \nEach incinerator line is provided with its own gas cleaning and monitoring equipment. Gas cleaning \ncomprises urea injection, activated carbon injection, semi-dry scrubbing using milk of lime spray followed by \nbag filters prior to discharge to atmosphere via two flues contained in one 47 m stack. Emissions from the \nstack are continuously monitored for particulates, carbon monoxide (CO), ammonia, sulphur dioxide (SO2), \nhydrogen chloride (HCl), oxygen (O2), nitrogen oxides (NOx) and volatile organic compounds (VOC). \nThere is no discharge of process liquids to controlled waters. Uncontaminated surface and roof waters are discharged to the surface water sewer system.",null,null,null,null,null,null,null,null,null,"Include summary of key processes and procedures such as (but not limited to); waste reception, control rooms, grate, bed and bolier, energy & heat  generation, cooling systems, residue management, emission controls, health and safety systems, maintenance"]

{"sheet":"Operational Data","index":3,"n_rows":65,"n_cols":11,"rows_kept":65,"cut":false,"hidden":false,"merged":[[52,0,56,0],[5,10,6,10],[7,10,18,10],[33,1,38,1],[3,1,3,2],[7,1,19,1],[23,1,26,1],[28,1,29,1]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Operational Data",null,null,null,null,null,null,null,null,null,"Notes:"]
["Plant Size","105'000",null,"tonnes pa",null,"MWth",7.14,"MWe",null,null,"* - RDF to include SRF "]
["No. of combustion lines",2,null,"No. of Turbines:",null,1,null,null,null,null,"** - CHP plants only"]
[null,null,null,null,null,null,null,null,null,null,"2020 updates include;  heat in MWh, water in Litres, NCV in MJ/kg"]
["Waste types received","Unit","Q1","Q2","Q3","Q4","Year Total","%"]
["Household / Local Authority","tonnes",11032.92,21288.19,17482.64,20549.689999999999,{"$f":"SUM(C8:F8)","v":70353.440000000002},{"$f":"IF(G8>0,G8/$G$18,\"-\")","v":0.92055194302199483},null,null,"Availabiity Definition: 'the availability of a line is to be calculated by the number of hours the line reported Continuously Monitored emission levels to the Regulator through the calendar year divided by the total number of hours in that year. \nThe overall plant availability is calculated as the Mean of all lines in the plant. For clarity this includes periods of Other Than Normal Operating Conditions (OTNOC) and abnormal operation.'  \n\nRationale: The primary function of an Energy from Waste facility is the disposal of waste. It follows therefore that the availability of a plant is determined by the period of time a facility spends undertaking this activity."]
["Commercial & Industrial ",null,1264.0999999999999,2645.67,717.92,1444.15,{"$f":"SUM(C9:F9)","v":6071.84},7.944805697800518E-2]
["Hazardous ",null,null,null,null,null,0,"-"]
["Clinical",null,null,null,null,null,0,"-"]
["Waste wood (biomass) ",null,null,null,null,null,0,"-"]
["Refuse Derived Fuel * - H'hold/LA",null,null,null,null,null,{"$f":"SUM(C13:F13)","v":0},"-"]
["Refuse Derived Fuel *  - C&I",null,null,null,null,null,0,"-"]
["Other [Please specify]",null,null,null,null,null,0,"-"]
["Other [Please specify]"]
["Other [Please specify]"]
["Total waste received",null,{"$f":"SUM(C8:C17)","v":12297.02},{"$f":"SUM(D8:D17)","v":23933.86},{"$f":"SUM(E8:E17)","v":18200.559999999998},{"$f":"SUM(F8:F17)","v":21993.84},{"$f":"SUM(G8:G17)","v":76425.279999999999},1]
["Rejected Waste ",null,null,null,null,null,{"$f":"SUM(C19:F19)","v":0},{"$f":"IF(G19>0,G19/$G$18,\"-\")","v":"-"}]
["Unprocessed waste transferred out",null,422.28,882.24,3963.12,1946.28,{"$f":"SUM(C20:F20)","v":7213.9199999999992},{"$f":"IF(G20>0,G20/$G$18,\"-\")","v":9.4391803340465347E-2}]
["Total waste combusted",null,{"$f":"C18-SUM(C19:C20)","v":11874.74},{"$f":"D18-SUM(D19:D20)","v":23051.62},14237.439999999999,20047.560000000001,{"$f":"SUM(C21:F21)","v":69211.360000000001},{"$f":"IF(G21>0,G21/$G$18,\"-\")","v":0.90560819665953463}]
[]
["Energy Useage / Export","Unit","Q1","Q2","Q3","Q4","Year Total","KWh/te"]
["Power Generated","MWh",8969.93,10148.84,6665.37,8012.41,{"$f":"SUM(C24:F24)","v":33796.550000000003},{"$f":"IF(G24>0,G24*1000/$G$21,\"-\")","v":488.30928911092053}]
["Power Exported",null,6653.9,7776.1,4929.6000000000004,6118.9,{"$f":"SUM(C25:F25)","v":25478.5},{"$f":"IF(G25>0,G25*1000/$G$21,\"-\")","v":368.12598394252041}]
["Power Used on site",null,2383.09,2412.84,2071.73,2127.77,{"$f":"SUM(C26:F26)","v":8995.43},{"$f":"IF(G26>0,G26*1000/$G$21,\"-\")","v":129.97042682010584}]
["Power Imported",null,67.06,40.1,335.96,234.25,677.37,{"$f":"IF(G27>0,G27*1000/$G$21,\"-\")","v":9.786977166754129}]
["Parasitic Load","%",{"$f":"IF(C24>0,1-C25/(C24+C27),\"-\")","v":0.26370395452468132},{"$f":"IF(D24>0,1-D25/(D24+D27),\"-\")","v":0.23680971720316346},{"$f":"IF(E24>0,1-E25/(E24+E27),\"-\")","v":0.29590520658217789},{"$f":"IF(F24>0,1-F25/(F24+F27),\"-\")","v":0.25801475991492318},{"$f":"IF(G24>0,1-G25/(G24+G27),\"-\")","v":0.2609340626189306}]
["Thermal Energy Produced **","MWh",null,null,null,null,{"$f":"SUM(C29:F29)","v":0},{"$f":"IF(G29>0,G29*1000/$G$21,\"-\")","v":"-"}]
["Thermal Energy Exported **",null,null,null,null,null,0,{"$f":"IF(G30>0,G30*1000/$G$21,\"-\")","v":"-"}]
["R1 value (if applicable)"]
[]
["Waste Disposal & Recovery","Unit","Q1","Q2","Q3","Q4","Year Total","% inputs"]
["APC Residues - produced","tonnes",316.64,751.62,483.86,647.55999999999995,{"$f":"SUM(C34:F34)","v":2199.6799999999998},{"$f":"IF(G34>0,G34/$G$21,\"-\")","v":3.1782065834279227E-2}]
["IBA - produced",null,1768.7,4148.1000000000004,2623.82,3587.65,12128.27,{"$f":"IF(G35>0,G35/$G$21,\"-\")","v":0.17523525039820054}]
["Metals recycling",null,195.44,430.54,273,170.78,{"$f":"SUM(C36:F36)","v":1069.76},1.5456422182716825E-2]
["Other",null,0,0,0,0,{"$f":"SUM(C37:F37)","v":0},"-"]
["Other",null,0,0,0,0,0,"-"]
["Other",null,0,0,0,0,0,"-"]
[]
["Raw Material Usage","Unit","Q1","Q2","Q3","Q4","Year Total","kg or Ltr /te"]
["Mains Water","ltrs",9012000,9311000,11527000,16664000,{"$f":"SUM(C42:F42)","v":46514000},{"$f":"IF(G42>0,G42/$G$21,\"-\")","v":672.05730388768552}]
["Other Water","ltrs",null,null,null,null,0,{"$f":"IF(G43>0,G43/$G$21,\"-\")","v":"-"}]
["Ammonia","kgs",null,null,null,null,0,"-"]
["Urea","kgs",15000,29000,33000,44000,{"$f":"SUM(C45:F45)","v":121000},1.7482679144001794]
["Activated Carbon","kgs",2000,3000,2000,2000,9000,0.13003645644298856]
["Lime / hydrated lime","kgs",111100,229120,164980,212160,717360,10.364772488215808]
["Fuel oil","ltrs",19186,10918,20767,23935,74806,1.0808341289638002]
["Gas","cf",0,0,0,0,0]
["Other",null,0,0,0,0,0]
[]
["Summary ","Line/Unit","Q1","Q2","Q3","Q4","Year Total",null,null,"Hrs in year "]
["Availability of waste combustion by line, hrs",1,1572.5,2116.4499999999998,1603.5,1827.26,{"$f":"SUM(C53:F53)","v":7119.71},0.81269999999999998,null,8760]
[null,2,1894.8,1901.65,1582.67,1864,7243.12,0.82679999999999998]
[null,3,null,null,null,null,0,"x %"]
[null,4,null,null,null,null,0,"x %"]
[null,5,null,null,null,null,{"$f":"SUM(C57:F57)","v":0},"x %"]
["Overall Availability, mean avg. of all lines, hrs",null,1734,2009,1593,1846,{"$f":"AVERAGE(G53:G54)","v":7181.415},0.81969999999999998]
["Hours of turbine operations, hrs",1,1912.5,2129.5500000000002,1406.5,1749.5,7198.05,0.82169999999999999]
["Hours of turbine operations, hrs",2,null,null,null,null,0,"x %"]
["Hours of heat / steam export",null,null,null,null,null,0,{"$f":"IF(B61>0,G60/J53,\"n/a\")","v":"n/a"}]
["Net Calorific Value of waste","MJ/kg",null,null,null,null,null,"-"]
["Abnormal Events","qty.",null,2,1,1,4,{"$f":"IF(G63>0,\"yes\",\"no\")","v":"yes"}]
["Abnormal operation","hours",null,16,1,0.5,17.5,{"$f":"+(G64)/J53","v":1.9977168949771688E-3}]
["Permit Breaches","qty.",1,5,3,4,13,{"$f":"IF(G65>0,\"yes\",\"no\")","v":"yes"}]

{"sheet":"Operational Summary","index":4,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[[4,0,26,8],[30,0,51,8],[4,10,13,13],[30,10,39,13]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Summary of Plant Operations and Maintenance during the reporting year",null,null,null,null,null,null,null,null,null,"Notes:"]
[]
["Both boilers were in operation for a cobined total of 14363 hours, with the turbine available for 7198 hours. Downtime included the annual outage along with smaller outages for boiler & maintenance issues",null,null,null,null,null,null,null,null,null,"Include summary of key operational and/or mainteanance activity undertaken in the year, such as any major component upgrades and/or replacements "]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Summary of Residue Handling for the reporting year"]
[]
["The facility has sent the majority bof IBA for processing and recycling in Derbyshire,  Ferrous to Doncaster. APCr has been sent to Peterborough.",null,null,null,null,null,null,null,null,null,"Include in here a summary of residue handling regimes and destinations "]

{"sheet":"Perf. Form 1","index":5,"n_rows":54,"n_cols":10,"rows_kept":54,"cut":false,"hidden":false,"merged":[[9,0,9,9],[10,0,10,1],[10,2,10,3],[10,4,10,5],[10,6,10,7],[10,8,10,9],[2,0,2,4],[2,6,2,8],[3,1,3,4],[5,3,5,4],[5,6,5,7],[8,0,8,1],[8,2,8,3],[8,4,8,5],[8,6,8,7],[8,8,8,9],[11,0,11,1],[11,2,11,3],[11,4,11,5],[11,6,11,7],[11,8,11,9],[12,0,12,1],[12,2,12,3],[12,4,12,5],[12,6,12,7],[12,8,12,9],[15,0,15,1],[15,2,15,3],[15,4,15,5],[15,6,15,7],[15,8,15,9],[16,0,16,9],[13,0,13,1],[13,2,13,3],[13,4,13,5],[13,6,13,7],[13,8,13,9],[14,0,14,3],[14,4,14,5],[14,6,14,7],[14,8,14,9],[17,0,17,1],[17,2,17,3],[17,4,17,5],[17,6,17,7],[17,8,17,9],[18,0,18,1],[18,2,18,3],[18,4,18,5],[18,6,18,7],[18,8,18,9],[19,0,19,1],[19,2,19,3],[19,4,19,5],[19,6,19,7],[19,8,19,9],[20,0,20,1],[20,2,20,3],[20,4,20,5],[20,6,20,7],[20,8,20,9],[21,0,21,1],[21,2,21,3],[21,4,21,5],[21,6,21,7],[21,8,21,9],[22,0,22,3],[22,4,22,5],[22,6,22,7],[22,8,22,9],[31,0,31,3],[31,7,31,8],[32,0,32,3],[32,4,32,5],[32,7,32,8],[33,0,33,3],[33,4,33,5],[33,7,33,8],[23,0,23,3],[23,4,23,5],[23,6,23,7],[23,8,23,9],[25,0,25,9],[26,0,28,9],[36,0,36,3],[36,4,36,5],[36,7,36,8],[37,0,37,3],[37,4,37,5],[37,7,37,8],[34,0,34,3],[34,4,34,5],[34,7,34,8],[35,0,35,3],[35,4,35,5],[35,7,35,8],[47,0,47,1],[49,0,49,9],[50,0,51,9],[38,0,38,9],[39,0,40,9],[43,0,43,1],[43,2,43,9],[45,0,45,1],[46,0,46,1]]}
[{"$f":"+'Cover Page'!C39","v":2023}," Annual Reporting Performance Form 1"]
[]
[{"$f":"+'Cover Page'!B31","v":"Permit EPR/HP3247QS"},null,null,null,null,"Operator: ",{"$f":"+'Cover Page'!B37:I37","v":0}]
["Facility:",{"$f":"+'Cover Page'!B33:I33","v":"Dudley Energy from Waste"},null,null,null,"Form:","Performance 1"]
[]
["Reporting  Period from: ",null,null,"2023-01-01",null,"to:","2023-12-31"]
[]
[{"$f":"+A1","v":2023},"Annual Reporting of Waste Disposal and Recovery"]
["Waste Description",null,"Disposal Route(s)",null,"Disposal Tonnes",null,"Recovery Tonnes",null,"% / tonne of waste incinerated"]
["1) Hazardous Wastes"]
["APC Residues",null,"East Northhamptonshire",null,2200,null,null,null,{"$f":"IF((E11+G11)>0,(E11+G11)/'Operational Data'!$G$21, \"-\")","v":3.1786689352730532E-2}]
["IBA",null,null,null,null,null,null,null,{"$f":"IF((E12+G12)>0,(E12+G12)/'Operational Data'!$G$21, \"-\")","v":"-"}]
[null,null,null,null,null,null,null,null,{"$f":"IF((E13+G13)>0,(E13+G13)/'Operational Data'!$G$21, \"-\")","v":"-"}]
[null,null,null,null,null,null,null,null,{"$f":"IF((E14+G14)>0,(E14+G14)/'Operational Data'!$G$21, \"-\")","v":"-"}]
["Total Hazardous Waste",null,null,null,{"$f":"SUM(E11:F14)","v":2200},null,{"$f":"SUM(G11:H14)","v":0},null,{"$f":"IF((E15+G15)>0,(E15+G15)/'Operational Data'!$G$21, \"-\")","v":3.1786689352730532E-2}]
[]
["2) Non-Hazardous Wastes"]
["IBA",null,"Derbyshire",null,null,null,12128,null,{"$f":"IF((E18+G18)>0,(E18+G18)/'Operational Data'!$G$21, \"-\")","v":0.17523134930450723}]
["Ferrous Metal",null,"Doncaster",null,null,null,1070,null,{"$f":"IF((E19+G19)>0,(E19+G19)/'Operational Data'!$G$21, \"-\")","v":1.5459889821555306E-2}]
["Process Water",null,null,null,null,null,null,null,{"$f":"IF((E20+G20)>0,(E20+G20)/'Operational Data'!$G$21, \"-\")","v":"-"}]
[null,null,null,null,null,null,null,null,{"$f":"IF((E21+G21)>0,(E21+G21)/'Operational Data'!$G$21, \"-\")","v":"-"}]
[null,null,null,null,null,null,null,null,{"$f":"IF((E22+G22)>0,(E22+G22)/'Operational Data'!$G$21, \"-\")","v":"-"}]
["Total Non-Hazardous Waste",null,null,null,{"$f":"SUM(E18:F22)","v":0},null,{"$f":"SUM(G18:H22)","v":13198},null,{"$f":"IF((E23+G23)>0,(E23+G23)/'Operational Data'!$G$21, \"-\")","v":0.19069123912606253}]
["TOTAL WASTE",null,null,null,{"$f":"+E23+E15","v":2200},null,{"$f":"+G23+G15","v":13198},null,{"$f":"IF((E24+G24)>0,(E24+G24)/'Operational Data'!$G$21, \"-\")","v":0.22247792847879308}]
[]
["Operator’s comments :"]
[]
[]
[]
[]
[{"$f":"+A1","v":2023},"Annual Reporting of Water and Other Raw Material Usage"]
["Raw Material",null,null,null,"Usage",null,"Unit","Specific Useage",null,"Unit"]
["Mains Water",null,null,null,{"$f":"+'Operational Data'!G42","v":46514000},null,"m3",{"$f":"IF(E33>0,E33/'Operational Data'!$G$21,\"-\")","v":672.05730388768552},null,"m3/te"]
["Total Water",null,null,null,{"$f":"+'Operational Data'!G43+'Operational Data'!G42","v":46514000},null,"m3",{"$f":"IF(E34>0,E34/'Operational Data'!$G$21,\"-\")","v":672.05730388768552},null,"m3/te"]
["Urea / Ammonia",null,null,null,{"$f":"+'Operational Data'!G45","v":121000},null,"kg",{"$f":"IF(E35>0,E35/'Operational Data'!$G$21,\"-\")","v":1.7482679144001794},null,"kg/te"]
["Activated Carbon",null,null,null,{"$f":"+'Operational Data'!G46","v":9000},null,"kg",{"$f":"IF(E36>0,E36/'Operational Data'!$G$21,\"-\")","v":0.13003645644298856},null,"kg/te"]
["Lime / hydrated lime / Sodium Bicarb.",null,null,null,{"$f":"+'Operational Data'!G47","v":717360},null,"kg",{"$f":"IF(E37>0,E37/'Operational Data'!$G$21,\"-\")","v":10.364772488215808},null,"kg/te"]
[]
["Operator’s comments :"]
[]
[]
[]
[{"$f":"+A31","v":2023},"Annual Reporting of other performance indicators "]
["Parameter",null,"Results by Line"]
[null,null,"A1","A2","A3","A4","A5",null,"Turbine 1","Turbine 2"]
["Operating hours for the year, hours",null,7120,7243]
["Number of periods of abnormal operation, qty.",null,1,3]
["Cumulative hours of abnormal operation for this year, hours",null,1,17]
[]
["Operator’s comments :"]
[]
[]
[]
["Signed: ","Carl Pearce",null,null,null,null,"Date:","2024-01-24"]

{"sheet":"Energy Form 1","index":6,"n_rows":29,"n_cols":8,"rows_kept":29,"cut":false,"hidden":false,"merged":[[2,6,2,8],[4,1,4,4],[6,3,6,4],[6,6,6,7],[8,0,8,2],[8,3,8,4],[8,6,8,8],[9,0,9,2],[9,3,9,4],[9,6,9,8],[10,0,10,2],[10,3,10,4],[10,6,10,8],[11,0,11,2],[11,3,11,4],[11,6,11,8],[12,0,12,2],[12,3,12,4],[12,6,12,8],[13,0,13,2],[13,3,13,4],[13,6,13,8],[14,0,14,2],[14,3,14,4],[14,6,14,8],[15,0,15,2],[15,3,15,4],[15,6,15,8],[17,0,17,8],[18,0,24,8]]}
[{"$f":"+'Cover Page'!C39","v":2023}," Annual Reporting of Energy Usage/Export"]
[]
[{"$f":"+'Cover Page'!B31","v":"Permit EPR/HP3247QS"},null,null,null,null,"Operator: ",{"$f":"+'Cover Page'!B37:I37","v":0}]
[]
["Facility:",{"$f":"+'Cover Page'!B33:I33","v":"Dudley Energy from Waste"},null,null,null,"Form:","Energy 1"]
[]
["Reporting  Period from: ",null,null,{"$f":"+'Perf. Form 1'!D6:E6","v":"2023-01-01"},null,"to:",{"$f":"+'Perf. Form 1'!G6:H6","v":"2023-12-31"}]
[]
["Energy Source",null,null,"Energy Usage",null,"Unit","Specific Useage (KWh/tonne incinerated"]
["Electricity Produced",null,null,{"$f":"+'Operational Data'!G24","v":33796.550000000003},null,"MWh",{"$f":"+'Operational Data'!H24","v":488.30928911092053}]
["Electricity Imported   ",null,null,{"$f":"+'Operational Data'!G27","v":677.37},null,"MWh",{"$f":"+'Operational Data'!H27","v":9.786977166754129}]
["Electricity Exported",null,null,{"$f":"+'Operational Data'!G25","v":25478.5},null,"MWh",{"$f":"+'Operational Data'!H25","v":368.12598394252041}]
["Gas Oil",null,null,64.33,null,"tonnes"]
["Steam/hot water exported",null,null,{"$f":"+'Operational Data'!G30","v":0},null,"GWh",{"$f":"+'Operational Data'!H30","v":"-"}]
[]
[]
[]
["Operator’s comments :"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Signed: ","Carl Pearce",null,null,null,null,"Date:","2024-01-24"]

{"sheet":"Permit Compliance","index":7,"n_rows":46,"n_cols":12,"rows_kept":46,"cut":false,"hidden":false,"merged":[[8,11,17,14],[45,4,45,8],[9,0,9,1],[9,2,9,4],[9,5,9,8],[10,0,10,1],[10,2,10,4],[10,5,10,8],[11,0,11,1],[11,2,11,4],[11,5,11,8],[12,0,12,1],[12,2,12,4],[12,5,12,8],[13,0,13,1],[13,2,13,4],[7,0,7,1],[7,2,7,8],[8,0,8,1],[8,2,8,4],[8,5,8,8],[13,5,13,8],[14,0,14,1],[14,2,14,4],[14,5,14,8],[15,0,15,1],[16,2,16,4],[16,5,16,8],[15,2,15,4],[15,5,15,8],[16,0,16,1],[19,1,19,3],[19,4,19,6],[19,7,19,9],[20,1,20,3],[20,4,20,6],[36,7,36,9],[21,1,21,3],[21,4,21,6],[34,1,34,3],[34,4,34,6],[34,7,34,9],[33,1,33,3],[22,7,22,9],[24,7,24,9],[25,7,25,9],[26,7,26,9],[27,7,27,9],[28,7,28,9],[29,7,29,9],[30,7,30,9],[31,7,31,9],[44,1,44,3],[44,4,44,6],[44,7,44,9],[41,1,41,3],[41,4,41,6],[41,7,41,9],[42,1,42,3],[42,4,42,6],[42,7,42,9],[38,0,38,10],[18,0,18,10],[43,1,43,3],[43,4,43,6],[43,7,43,9],[39,1,39,3],[39,4,39,6],[39,7,39,9],[40,1,40,3],[40,4,40,6],[40,7,40,9],[35,1,35,3],[35,4,35,6],[35,7,35,9],[36,1,36,3],[36,4,36,6],[32,7,32,9],[23,7,23,9],[24,1,24,3],[24,4,24,6],[25,4,25,6],[26,4,26,6],[32,4,32,6],[33,4,33,6],[22,1,22,3],[22,4,22,6],[23,1,23,3],[23,4,23,6],[27,4,27,6],[28,1,28,3],[28,4,28,6],[29,4,29,6],[30,4,30,6],[31,4,31,6]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Summary of Permit Compliance"]
[]
["Compliance with permit limits for continuously monitored pollutants"]
[]
["The plant met its emission limits as shown in the table below:"]
["Substance",null,"Percentage time compliant during operation",null,null,null,null,null,null,null,null,"Notes:"]
[null,null,"Half-hourly limit",null,null,"Daily limit",null,null,null,null,null,"Report to 2 decimal places, i.e. xx.xx%\n\nPlease provide a brief summary of each notification or non-compliance in the table (rather than just referring to notifications that were sent to the Regulator).  \n\n"]
["Particulates",null,99.99,null,null,100]
["Oxides of nitrogen",null,99.99,null,null,99.67]
["Sulphur dioxide",null,99.99,null,null,100]
["Carbon monoxide",null,99.96,null,null,100]
["Total organic carbon",null,99.98,null,null,100]
["Hydrogen chloride",null,99.98,null,null,99.5]
["Hydrogen fluoride",null,100,null,null,100]
["NH3",null,"N/A",null,null,97.64]
[]
["Summary of any notifications or non-compliances under the permit"]
["Date","Summary of notification or non-compliance [including Line/Reference]",null,null,"Reason ",null,null,"Measures taken to prevent reoccurrence"]
["2023-03-12","A2 - HCL Daily Limit 10.5 mg/m3",null,null,"Lime Flow Meter Broken",null,null,"Quote for new flow meter Submitted to DMBC for approval"]
["2023-04-12","A1 - HCL Daily Limit 10.01 mg/m3",null,null,"Lime Flow Meter Broken",null,null,"Quote for new flow meter Submitted to DMBC for approval"]
["2023-04-13","A1 - HCL Half Hour Limit 97.43 mg/m3",null,null,"Lime Flow Meter Broken",null,null,"Quote for new flow meter Submitted to DMBC for approval"]
["2023-04-16","A1 - HCL & SO2 Half Hour Limits 106.90 mg/m3 & 217.60 mg/m3 respectively",null,null,"Lime Flow Meter Broken",null,null,"Quote for new flow meter Submitted to DMBC for approval"]
["2023-04-18","A1 - HCL Half Hour Limits 73.43 mg/m3 & 123.89 mg/m3 - A2 - HCL Half Hour Limit  127.24 mg/m3",null,null,"Lime Flow Meter Broken",null,null,"Quote approved by DMBC. Flow meter ordered 6 weeks delivery."]
["2023-05-04","A1 - HCL Half Hour Limit 84.33 mg/m3",null,null,"Lime Flow Meter Broken",null,null,"Quote approved by DMBC. Flow meter ordered 4 weeks delivery."]
["2023-06-21","A2 - HCL Daily Limit 74.04 mg/m3",null,null,"Lime Turbine Belt Split",null,null,"New Lime Turbine Belt fitted within 1/2 hour."]
["2023-06-30","A2 - VOC Half Hour Limit 40.90 mg/m3 ",null,null,"Super Heater Transmitter Failed",null,null,"Super Heater Transmitter repaired & new parts sourced."]
["2023-07-03","A1 - Nox Half Hour Limit 464.51 mg/m3 & VOC Half Hour Limit 149.30 mg/m3 ",null,null,"Ash Discharger Blocked causing interlock within system to stop A1 feeder to boiler",null,null,"Ash Discharger Un-blocked within 1/2 hour & A1 feeder back running."]
["2023-07-31","A2 - HCL Daily Limit 10.14 mg/m3",null,null,"Problem with Lime Turbine",null,null,"Lime Turbine Changed"]
["2023-08-11","A2 - Nox Half Hour Limits 452.91 mg/m3, 593.09 mg/m3 & VOC Half Hour Limit 51.46 mg/m3",null,null,"Grate feeding boiler 2 blocked causing Boiler 2 to trip.",null,null,"Boiler 2 taken off-line to start annual outage early."]
["2023-09-04","A2 - Particulates Half Hour Limits 30.97 mg/m3  & 31.42 mg/m3",null,null,"Bringing Boiler 2 back on line after outage particulate increase at start of burning & feed pumps tripped.",null,null,"Kept boiler 2 off & re-started on 5/09/23"]
["2023-11-06","A1 - Nox Half Hour Limit 501.23 mg/m3 , 497.03 mg/m3 & VOC Half Hour Limit 47.04 mg/m3  & 54.95mg/m3. CO = 16 x 10 minutes - A2=  CO 14 x 10 minutes",null,null,"Wet waste fed into boilers.",null,null,"Re-lit burners & under fire air, mixed wet waste with new dry waste."]
["2023-11-13","A1 = CO 1 x 10 minute & A2 = CO 3 x 10 minute",null,null,"Wet waste fed into boilers.",null,null,"Re-lit burners & under fire air, mixed wet waste with new dry waste."]
["2023-12-10","A1 - Nox Daily  182.21 mg/m3, NH3 Daily Limit 15.10 mg/m3 &  VOC Half Hour Limit 185.79 mg/m3",null,null,"Lost steam flow on boiler 1",null,null,"Burber re-lit & steam flow back under control"]
["2023-12-13","A2 - Nox Daily Limit 187.01 mg/m3",null,null,"Bang & Clean caused temperature to drop resulting in high Nox",null,null,"Bang & clean suspended"]
["2023-12-14","A1 - SO2 Half Hour Limit 218.30 mg/m3",null,null,"Lime pump feeding boiler 1 blocked",null,null,"Unblocked within half hour."]
[]
["Summary of any complaints received and actions to taken to resolve them."]
["Date","Summary of complaint [including Line/Reference]",null,null,"Reason *",null,null,"Measures taken to prevent reoccurrence"]
[]
[]
[]
[]
[]
[null,null,null,null,"* including whether substantiated by the operator or the EA"]

{"sheet":"Improvements","index":8,"n_rows":38,"n_cols":5,"rows_kept":38,"cut":false,"hidden":false,"merged":[[37,0,37,8],[38,0,47,8],[4,0,4,8],[5,0,13,8],[15,0,15,8],[16,0,24,8],[26,0,26,8],[27,0,35,8]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Summary of Plant Improvements"]
[]
["Summary of any efficiency improvements that have been completed within the year."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Summary of any permit improvement conditions that have been completed within the year and the resulting environmental benefits."]
["Dioxin and mercury moniotring protocols have been followed to determine that the facility does not require CEMS for these two gases.\n\nReduction of NOx tests have been carried out to determine how low could be possible, however there isn't much room to further reduce the NOx levels due to the related ammonia emissions."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Summary of any changes to the plant or operating techniques which required a variation to the permit and a summary of the resulting environmental impact."]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Summary of any other improvements made to the plant or planned to be made and a summary of the resulting environmental benefits."]

{"sheet":"Public Liasion","index":9,"n_rows":29,"n_cols":5,"rows_kept":29,"cut":false,"hidden":false,"merged":[[16,0,16,1],[16,2,16,8],[5,0,5,1],[5,2,5,8],[6,0,7,1],[6,2,7,8],[8,0,9,1],[8,2,9,8],[10,0,11,1],[10,2,11,8],[12,0,13,1],[12,2,13,8],[15,0,15,8],[17,0,18,1],[17,2,18,8],[19,0,20,1],[19,2,20,8],[21,0,22,1],[21,2,22,8],[23,0,24,1],[23,2,24,8],[25,0,26,1],[25,2,26,8],[28,0,28,8]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Details of Public & Stakeholder Liasion"]
[]
["Summary of events held during the reporting year."]
["Date",null,"Description"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["List of events planned for next year"]
["Date",null,"Description"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["If you wish to be involved in the public liasion programme, please contact _________________"]

{"sheet":"CO2 N2O","index":10,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[[19,4,19,14],[17,4,17,14],[12,4,12,14],[8,4,8,14],[19,1,19,2],[22,0,23,2],[4,0,4,2],[8,1,8,2],[10,0,10,2],[12,1,12,2],[15,0,15,2],[17,1,17,2]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Carbon dioxide emissions and biogenic content of waste inputs",null,null,null,"Notes:"]
[]
["Carbon dioxide emissions (all types of plant)"]
["Annual mass of carbon dioxide released","x tonnes ",266160.71000000002]
["Annual mass of carbon dioxide released per tonne of waste burned","x tonnes ",3.85]
["Annual mass of carbon dioxide released per MWh of energy exported","x tonnes ",10.45]
["Description of how annual carbon dioxide mass emission has been calculated","Data found from CO2 CEMS ",null,null,"Note 1: Where available, data from CO2 CEMS should be used. Otherwise, where no CEMS data is available, a suitable emissions factor should be used based on the tonnage of waste burned e.g.0.992 tCO2/t waste as per Tolvik report 2021, or other justified emissions factor  - refer to embedded Environment Agency guidance note above or updated version for suitable descriptive text."]
[]
["Nitrous oxide emissions (only plants which use ammonia or urea to abate NOx emissions)"]
["Annual mass emissions of nitrous oxide","x tonnes ",10.099]
["Description of how annual nitrous oxide mass emission has been calculated","Data found from N2O CEMS",null,null,"Note 2: Where available, data from N2O CEMS should be used, or if no CEMS data is available, from periodic monitoring. Otherwise, a suitable emissions factor should be used based on the tonnage of waste burned e.g. 0.0981 kgN20/t waste as per 2021 Pollution Inventory data for plants with urea-based SNCR - refer to embedded Environment Agency guidance note above or updated version for suitable descriptive text."]
["Total annual carbon dioxide and nitrous oxide emissions as carbon dioxide equivalent (whereby 1 t nitrous oxide is equivalent to 298 t carbon dioxide)","x tonnes CO2e",269170.21000000002]
[]
["Biogenic fraction of the waste and biogenic CO2 emissions (only plants burning residual municipal waste, refuse derived fuel or solid recovered fuel)"]
["Yearly average biogenic percentage of the waste by net calorific value (NCV)","x %",60.3]
["Description of how biogenic NCV percentage has been calculated or estimated","Waste sampling by Socotec in accordance with UKAS schedule No: 0001",null,null,"Note 3: Where available, data from waste sampling should be used; otherwise, an estimated figure with justification can be used, or a figure assumed on the basis of a national average e.g. 2017 WRAP data for residual waste of 51.8% biogenic energy content - refer to embedded Environment Agency guidance note above or updated version for suitable descriptive text, quoting standards where relevant. "]
["Percentage of total carbon dioxide emissions arising from biogenic waste","x %",60.3]
["Description of how percentage biogenic carbon dioxide emissions have been calculated","Estimated biogenic fraction by net calorific value assumed as the bogenic CO2 fraction of the total CO2 emissions from the plant.",null,null,"Note 4: Examples include direct measurement via C14 method or BIOMA software - refer to embedded Environment Agency guidance note above or updated version for suitable descriptive text, quoting standards where relevant. Otherwise, as an approximation (and in lieu of any more accurate metrics which may be developed in future), the measured or estimated biogenic fraction by net calorific value can be assumed to be the same as the biogenic CO2 fraction of the total CO2 emissions from the plant. "]
[]
["Comments:"]

{"sheet":"Residue Quality ","index":11,"n_rows":36,"n_cols":6,"rows_kept":36,"cut":false,"hidden":false,"merged":[[16,0,17,1],[16,2,17,6],[18,0,19,1],[18,2,19,6],[12,0,12,6],[13,0,13,1],[13,2,13,6],[5,0,6,6],[7,0,8,6],[9,0,10,6],[14,0,15,1],[14,2,15,6],[20,0,21,1],[20,2,21,6],[22,0,23,1],[22,2,23,6],[31,3,31,4],[27,2,28,2],[28,3,28,4],[28,5,28,6],[27,3,27,6],[26,0,26,6],[35,0,40,6],[32,3,32,4],[34,0,34,6],[27,0,28,1],[29,0,29,1],[30,0,30,1],[31,0,31,1],[32,0,32,1],[29,3,29,4],[30,3,30,4],[29,5,29,6],[30,5,30,6],[31,5,31,6],[32,5,32,6]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Residue Quality Monitoring Requirements"]
[]
["Summary of monitoring undertaken and compliance"]
["From taking over the facility in February, twice monthly IBA core hazard assessment following the ESA protocol wuth an annual full hazardous assessment"]
[]
["All samples remained non-hazardous and compliant. Will continue the testing regime into the future."]
[]
[]
[]
[]
["Commentary on any specific events"]
["Date & Event",null,"Description"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["Residue Quality Monitoring Results"]
["Parameter (unit) ",null,"Limit","Normal Operation "]
[null,null,null,"Bottom ash  ",null,"APC Residues"]
["Loss on Ignition (average %)",null,"<5%","N/A"]
["Total Organic Carbon (average %)",null,"<3%",1.81]
["No. of Assessments Undertaken",null,"---",19,null,4]
["No. of Hazardous Results",null,"---",0]
[]
["Comments :"]
["No hazardous results identified on the twice monthly samples."]

{"sheet":"Water","index":12,"n_rows":23,"n_cols":9,"rows_kept":23,"cut":false,"hidden":false,"merged":[[5,0,6,8],[7,0,8,8],[9,0,10,8],[12,0,12,8],[13,0,13,1],[13,2,13,8],[21,0,21,8],[22,0,22,2],[22,3,22,4],[14,0,15,1],[14,2,15,8],[16,0,17,1],[16,2,17,8],[18,0,19,1],[18,2,19,8],[23,0,23,2],[23,3,23,4],[24,0,24,2],[24,3,24,4],[25,0,25,2],[25,3,25,4],[29,0,29,2],[29,3,29,4],[26,0,26,2],[26,3,26,4],[27,0,27,2],[27,3,27,4],[28,0,28,2],[28,3,28,4]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Emissions to Water"]
[]
["Summary of monitoring undertaken and compliance"]
[]
[]
[]
[]
[]
[]
[]
["Commentary on any specific events"]
["Date & Event",null,"Description"]
[]
[]
[]
[]
[]
[]
[]
["Emissions to Water / Sewer"]
["Parameter",null,null,"Monitoring Frequency",null,"Limit","Target","Max.","Average"]

{"sheet":"Air (periodic)","index":13,"n_rows":39,"n_cols":13,"rows_kept":39,"cut":false,"hidden":false,"merged":[[5,12,8,15],[9,12,11,15],[8,0,8,9],[5,0,6,9],[11,0,11,1],[12,0,12,1],[11,3,11,4],[12,3,12,4],[9,0,10,1],[9,5,9,9],[9,3,10,4],[9,2,10,2],[16,0,16,1],[17,0,17,1],[18,0,18,1],[13,0,13,1],[14,0,14,1],[15,0,15,1],[39,0,40,9],[25,0,25,1],[26,0,26,1],[22,0,22,1],[23,0,23,1],[37,0,37,1],[27,0,27,1],[28,0,28,1],[29,0,29,1],[30,0,30,1],[31,0,31,1],[32,0,32,1],[37,3,37,4],[29,3,29,4],[30,3,30,4],[36,3,36,4],[38,0,38,9],[19,0,19,1],[20,0,20,1],[21,0,21,1],[34,3,34,4],[35,3,35,4],[33,0,33,1],[34,0,34,1],[35,0,35,1],[36,0,36,1],[24,0,24,1],[32,3,32,4],[13,3,13,4],[14,3,14,4],[15,3,15,4],[16,3,16,4],[17,3,17,4],[18,3,18,4],[27,3,27,4],[33,3,33,4],[19,3,19,4],[20,3,20,4],[21,3,21,4],[22,3,22,4],[23,3,23,4],[24,3,24,4],[31,3,31,4],[25,3,25,4],[26,3,26,4],[28,3,28,4]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Emissions to Air (periodically monitored)"]
[]
["Summary of monitoring undertaken, standards used and compliance",null,null,null,null,null,null,null,null,null,null,null,"Notes:"]
["Two sets of monitoring throughout year by Socotec following standard EN14181",null,null,null,null,null,null,null,null,null,null,null,"Template may require adjustment for any bespoke monitoring requirements of permit. "]
[]
[]
["Results of emissions to air that are periodically monitored"]
["Substance",null,"Ref. Period","Emission Limit Value",null,"Average",null,null,null,null,null,null,"User to add additional tables as necessary, depending on whether quarterly or bi-annual reporting is required for the compliance year"]
[null,null,null,null,null,"A1","A2","A3","A4","A5"]
["Hydrogen fluoride",null,"1 hr","2 mg/m3",null,0.06,0.02]
["Cd and Th and their compounds",null,"6-8hrs","0.05 mg/m3",null,8.9999999999999998E-4,8.9999999999999998E-4]
["Hg and its compounds",null,"6-8hrs","0.05 mg/m3",null,3.8999999999999998E-3,2.7000000000000001E-3]
["Sb, As, Pb, Cr, Co, Cu, Mn, Ni, V and their compounds",null,"6-8hrs","0.5 mg/m3",null,5.7000000000000002E-2,3.6999999999999998E-2]
["Dioxins & Furans (I-TEQ)",null,"6-8hrs","0.1 ng/m3",null,2.2200000000000001E-2,0.02]
["PCBs (WHO-TEQ Humans / Mammals)",null,"6-8hrs","None set ng/m3",null,1.1299999999999999E-2,1.0500000000000001E-2]
["PCBs (WHO-TEQ Fish)",null,"6-8hrs","None set ng/m3",null,1E-4,0.01]
["PCBs (WHO-TEQ Birds)",null,"6-8hrs","None set ng/m3",null,5.5999999999999999E-3,1.5800000000000002E-2]
["Dioxins & Furans (WHO-TEQ Humans / Mammals)",null,"6-8hrs","None set ng/m3",null,1.3100000000000001E-2,1.0999999999999999E-2]
["Dioxins & Furans (WHO-TEQ Fish)",null,"6-8hrs","None set ng/m3",null,1.2500000000000001E-2,1.12E-2]
["Dioxins & Furans (WHO-TEQ Birds)",null,"6-8hrs","None set ng/m3",null,2.12E-2,2.0400000000000001E-2]
["Anthanthrene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Benzo(a)anthracene",null,"6-8hrs","None set µg/m3",null,1.4E-3,0]
["Benzo(a)pyrene",null,"6-8hrs","None set µg/m3",null,1.4E-3,0]
["Benzo(b)fluoranthene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Benzo(b)naptho(2,1-d) thiophene",null,"6-8hrs","None set µg/m3",null,1.4E-3,0]
["Benzo(c)phenanthrene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Benzo(ghi)perylene",null,"6-8hrs","None set µg/m3",null,1.4E-3,0.01]
["Benzo(k)fluoranthene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Cholanthrene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Chrysene",null,"6-8hrs","None set µg/m3",null,1.4E-3,0]
["Cyclopenta(cd)pyrene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Dibenzo(ai)pyrene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Dibenzo(ah)anthracene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Fluoranthene",null,"6-8hrs","None set µg/m3",null,0.01,7.0000000000000007E-2]
["Indeno(123-cd) pyrene",null,"6-8hrs","None set µg/m3",null,1.4E-3,1.4E-3]
["Naphthalene",null,"6-8hrs","None set µg/m3",null,0.21,9.64]
["Comments :"]

{"sheet":"Air (CEMS)","index":14,"n_rows":29,"n_cols":16,"rows_kept":29,"cut":false,"hidden":false,"merged":[[27,0,27,12],[29,0,30,12],[13,0,14,0],[5,0,6,12],[7,0,8,12],[10,0,10,12],[11,0,12,0],[11,2,12,2],[11,1,12,1],[11,3,11,4],[11,5,11,6],[11,7,11,8],[11,9,11,10],[11,11,11,12]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,null,null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Emissions to Air (continously monitored)"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Notes:"]
["Summary of monitoring undertaken, standards used and compliance",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Template may require adjustment for any bespoke monitoring requirements of permit"]
["Continuous monitoring from CEMS equipment",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Report to 2 decimal places, i.e. xx.xx%"]
[]
[]
[]
[]
["Results of emissions to air that are continuously monitored (maximum and average values for each line)"]
["Substance","Reference Period","Emission Limit Value","A1",null,"A2",null,"A3",null,"A4",null,"A5"]
[null,null,null,"Max.","Avg.","Max.","Avg.","Max.","Avg.","Max.","Avg.","Max.","Avg."]
["Oxides of nitrogen","Daily mean","200 mg/m3 ",200,176.98,190,179.15]
[null,"½ hourly mean","400 mg/m3 ",501,162,593,179.09]
["Particulates","Daily mean","10 mg/m3",2,0.4,3,1.1100000000000001]
[null,"½ hourly mean","30 mg/m3 ",24,0.25,31,1.0900000000000001]
["Total Organic Carbon ","Daily mean","10 mg/m3 ",5,0.97,3,0.51]
[null,"½ hourly mean","20 mg/m3 ",186,0.92,51,1]
["Hydrogen chloride ","Daily mean","10 mg/m3 ",10,5.65,11,5.73]
[null,"½ hourly mean","60 mg/m3 ",124,5.25,127,5.73]
["Sulphur dioxide","Daily mean","50 mg/m3 ",35,13.12,27,11.15]
[null,"½ hourly mean","200 mg/m3 ",218,11.92,176,11.18]
["Carbon monoxide ","Daily mean","50 mg/m3 ",176,7.81,112,17.53]
[]
[null,"95%ile 10-min avg *","150 mg/m3 *",1385,7.08,4048,16.91]
[" Ammonia","Daily mean","No limit set",54,9.27,31,9.3000000000000007]
["* = delete or amend as appropriate"]
["Comments :"]

{"sheet":"HCl","index":15,"n_rows":79,"n_cols":17,"rows_kept":79,"cut":false,"hidden":false,"merged":[[12,16,15,18],[51,9,63,9],[66,9,78,9],[4,9,4,14],[4,1,4,3],[4,4,4,6],[48,0,51,6],[47,0,47,6],[6,9,18,9],[21,9,33,9],[36,9,48,9],[3,16,7,18],[9,16,11,18]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Monitoring of Hydrogen Chloride emissions",null,null,"Whole Installation",null,null,"See  Notes in Cell Q3",null,null,{"$f":"+A3","v":"Monitoring of Hydrogen Chloride emissions"},null,null,null,"Per Combustion Line",null,null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User to add logic to complete Whole installation, Table A5:G18. From the data in Per Combustion Line, Table J6:O79, subject to No. of lines installed"]
["mg/Nm3","1/2 Hourly Reference Periods",null,null,"Daily Reference Periods"]
[{"$f":"+'Cover Page'!C39","v":2023},"1/2 hourly HCl ELV","Monthly 1/2 hourly mean","Highest 1/2 hourly maximum","Daily HCl ELV","Monthly daily mean","Highest daily maximum",null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
["Jan",60,null,null,10,null,null,null,null,"A1","Jan"]
["Feb",60,6.5,38,10,6.55,9,null,null,null,"Feb",7,38,6.7,9]
["Mar",60,7,46,10,6.99,11,null,null,null,"Mar",7,40,6.87,9,null,"Whole Installation table A5:G18:"]
["Apr",60,7,127,10,7.03,10,null,null,null,"Apr",7,124,7.2,10,null,"Mean: for 1/2 hourly and daily periods calculate mean of values across all operational combustion lines for the month"]
["May",60,6.5,88,10,6.41,8,null,null,null,"May",6,84,5.97,8]
["Jun",60,6.5,74,10,6.62,9,null,null,null,"Jun",6,31,6.46,9]
["Jul",60,7.5,46,10,7.41,10,null,null,null,"Jul",8,46,7.58,9,null,"Maximum: for 1/2 hourly and daily periods use the highest value across all operational combustion lines for the month"]
["Aug",60,7.5,27,10,7.35,8,null,null,null,"Aug",8,27,7.73,8]
["Sep",60,3.5,34,10,3.57,6,null,null,null,"Sep",3,34,3.27,6]
["Oct",60,4,31,10,3.68,6,null,null,null,"Oct",4,22,3.64,5]
["Nov",60,3.5,23,10,3.26,5,null,null,null,"Nov",4,23,3.62,5]
["Dec",60,3.5,45,10,3.72,6,null,null,null,"Dec",3,28,3.1,4]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L7:L18)","v":5.7272727272727275},{"$f":"MAX(M7:M18)","v":124},{"$f":"AVERAGE(N7:N18)","v":5.6490909090909085},{"$f":"MAX(O7:O18)","v":10}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A2","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb",6,31,6.4,8]
[null,null,null,null,null,null,null,null,null,null,"Mar",7,46,7.1,11]
[null,null,null,null,null,null,null,null,null,null,"Apr",7,127,6.85,10]
[null,null,null,null,null,null,null,null,null,null,"May",7,88,6.84,8]
[null,null,null,null,null,null,null,null,null,null,"Jun",7,74,6.78,8]
[null,null,null,null,null,null,null,null,null,null,"Jul",7,46,7.24,10]
[null,null,null,null,null,null,null,null,null,null,"Aug",7,24,6.96,8]
[null,null,null,null,null,null,null,null,null,null,"Sep",4,23,3.86,6]
[null,null,null,null,null,null,null,null,null,null,"Oct",4,31,3.72,6]
[null,null,null,null,null,null,null,null,null,null,"Nov",3,19,2.89,5]
[null,null,null,null,null,null,null,null,null,null,"Dec",4,45,4.34,6]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L22:L33)","v":5.7272727272727275},{"$f":"MAX(M22:M33)","v":127},{"$f":"AVERAGE(N22:N33)","v":5.7254545454545456},{"$f":"MAX(O22:O33)","v":11}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A3","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
["Comments :",null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L37:L48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M37:M48)","v":0},{"$f":"AVERAGE(N37:N48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O37:O48)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A4","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L52:L63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M52:M63)","v":0},{"$f":"AVERAGE(N52:N63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O52:O63)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A5","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L67:L78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M67:M78)","v":0},{"$f":"AVERAGE(N67:N78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O67:O78)","v":0}]

{"sheet":"SO2","index":16,"n_rows":79,"n_cols":17,"rows_kept":79,"cut":false,"hidden":false,"merged":[[3,16,7,18],[9,16,11,18],[12,16,15,18],[66,9,78,9],[4,1,4,3],[4,4,4,6],[4,9,4,14],[6,9,18,9],[21,9,33,9],[36,9,48,9],[47,0,47,6],[48,0,51,6],[51,9,63,9]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Monitoring of Sulphur dioxide emissions",null,null,"Whole Installation",null,null,"See  Notes in Cell Q3",null,null,{"$f":"+A3","v":"Monitoring of Sulphur dioxide emissions"},null,null,null,"Per Combustion Line",null,null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User to add logic to complete Whole installation, Table A5:G18. From the data in Per Combustion Line, Table J6:O79, subject to No. of lines installed"]
["mg/Nm3","1/2 Hourly Reference Periods",null,null,"Daily Reference Periods"]
[{"$f":"+'Cover Page'!C39","v":2023},"1/2 hourly SO2 ELV","Monthly 1/2 hourly mean","Highest 1/2 hourly maximum","Daily SO2 ELV","Monthly daily mean","Highest daily maximum",null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
["Jan",200,null,null,50,null,null,null,null,"A1","Jan"]
["Feb",200,7,46,50,6.79,15,null,null,null,"Feb",8,45,7.77,15]
["Mar",200,9.5,188,50,9.6300000000000008,29,null,null,null,"Mar",11,188,10.82,29,null,"Whole Installation table A5:G18:"]
["Apr",200,8,218,50,8.11,19,null,null,null,"Apr",9,218,9.14,19,null,"Mean: for 1/2 hourly and daily periods calculate mean of values across all operational combustion lines for the month"]
["May",200,9.5,123,50,9.5,17,null,null,null,"May",10,123,9.75,17]
["Jun",200,7,41,50,6.7,12,null,null,null,"Jun",6,41,6.38,12]
["Jul",200,8.5,119,50,8.52,14,null,null,null,"Jul",10,119,10.35,14,null,"Maximum: for 1/2 hourly and daily periods use the highest value across all operational combustion lines for the month"]
["Aug",200,12.5,60,50,13,20,null,null,null,"Aug",13,45,13.46,14]
["Sep",200,17,126,50,17.3,30,null,null,null,"Sep",15,126,15.2,30]
["Oct",200,14.5,94,50,14.39,27,null,null,null,"Oct",14,94,14.09,27]
["Nov",200,17.5,87,50,17.36,29,null,null,null,"Nov",22,87,21.95,29]
["Dec",200,22,218,50,22.1,35,null,null,null,"Dec",25,218,25.46,35]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L7:L18)","v":13},{"$f":"MAX(M7:M18)","v":218},{"$f":"AVERAGE(N7:N18)","v":13.124545454545457},{"$f":"MAX(O7:O18)","v":35}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A2","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb",6,46,5.81,9]
[null,null,null,null,null,null,null,null,null,null,"Mar",8,79,8.43,18]
[null,null,null,null,null,null,null,null,null,null,"Apr",7,101,7.08,12]
[null,null,null,null,null,null,null,null,null,null,"May",9,90,9.25,15]
[null,null,null,null,null,null,null,null,null,null,"Jun",8,39,7.53,12]
[null,null,null,null,null,null,null,null,null,null,"Jul",7,43,6.69,10]
[null,null,null,null,null,null,null,null,null,null,"Aug",12,60,12.45,20]
[null,null,null,null,null,null,null,null,null,null,"Sep",19,107,19.309999999999999,23]
[null,null,null,null,null,null,null,null,null,null,"Oct",15,59,14.68,19]
[null,null,null,null,null,null,null,null,null,null,"Nov",13,80,12.77,27]
[null,null,null,null,null,null,null,null,null,null,"Dec",19,176,18.649999999999999,27]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L22:L33)","v":11.181818181818182},{"$f":"MAX(M22:M33)","v":176},{"$f":"AVERAGE(N22:N33)","v":11.149999999999999},{"$f":"MAX(O22:O33)","v":27}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A3","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
["Comments :",null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L37:L48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M37:M48)","v":0},{"$f":"AVERAGE(N37:N48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O37:O48)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A4","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L52:L63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M52:M63)","v":0},{"$f":"AVERAGE(N52:N63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O52:O63)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A5","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L67:L78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M67:M78)","v":0},{"$f":"AVERAGE(N67:N78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O67:O78)","v":0}]

{"sheet":"NOx","index":17,"n_rows":79,"n_cols":17,"rows_kept":79,"cut":false,"hidden":false,"merged":[[3,16,7,18],[9,16,11,18],[12,16,15,18],[66,9,78,9],[4,1,4,3],[4,4,4,6],[4,9,4,14],[6,9,18,9],[21,9,33,9],[36,9,48,9],[47,0,47,6],[48,0,51,6],[51,9,63,9]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Monitoring of Oxides of Nitrogen emissions",null,null,"Whole Installation",null,null,"See  Notes in Cell Q3",null,null,{"$f":"+A3","v":"Monitoring of Oxides of Nitrogen emissions"},null,null,null,"Per Combustion Line",null,null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User to add logic to complete Whole installation, Table A5:G18. From the data in Per Combustion Line, Table J6:O79, subject to No. of lines installed"]
["mg/Nm3","1/2 Hourly Reference Periods",null,null,"Daily Reference Periods"]
[{"$f":"+'Cover Page'!C39","v":2023},"1/2 hourly NOx ELV","Monthly 1/2 hourly mean","Highest 1/2 hourly maximum","Daily NOx ELV","Monthly daily mean","Highest daily maximum",null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
["Jan",400,null,null,200,null,null,null,null,"A1","Jan"]
["Feb",400,179,270,200,179.26,181,null,null,null,"Feb",179,252,179.09,181]
["Mar",400,180,336,200,180.19,185,null,null,null,"Mar",180,291,180.1,184,null,"Whole Installation table A5:G18:"]
["Apr",400,180,309,200,180.2,186,null,null,null,"Apr",180,309,180.28,186,null,"Mean: for 1/2 hourly and daily periods calculate mean of values across all operational combustion lines for the month"]
["May",400,180.5,342,200,180.36,190,null,null,null,"May",180,236,179.86,182]
["Jun",400,179.5,313,200,179.49,184,null,null,null,"Jun",179,228,178.63,181]
["Jul",400,178,465,200,177.98,186,null,null,null,"Jul",180,465,180.14,186,null,"Maximum: for 1/2 hourly and daily periods use the highest value across all operational combustion lines for the month"]
["Aug",400,171,593,200,171.41,181,null,null,null,"Aug",156,186,156.33000000000001,174]
["Sep",400,181.5,400,200,181.32,186,null,null,null,"Sep",182,400,181.71,186]
["Oct",400,174.5,303,200,174.2,183,null,null,null,"Oct",176,301,175.8,183]
["Nov",400,178,501,200,178.08,200,null,null,null,"Nov",178,501,178.42,200]
["Dec",400,176,390,200,176.21,187,null,null,null,"Dec",176,390,176.37,182]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L7:L18)","v":176.90909090909091},{"$f":"MAX(M7:M18)","v":501},{"$f":"AVERAGE(N7:N18)","v":176.97545454545454},{"$f":"MAX(O7:O18)","v":200}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A2","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb",179,270,179.43,180]
[null,null,null,null,null,null,null,null,null,null,"Mar",180,336,180.27,185]
[null,null,null,null,null,null,null,null,null,null,"Apr",180,281,180.11,185]
[null,null,null,null,null,null,null,null,null,null,"May",181,342,180.86,190]
[null,null,null,null,null,null,null,null,null,null,"Jun",180,313,180.34,184]
[null,null,null,null,null,null,null,null,null,null,"Jul",176,243,175.81,183]
[null,null,null,null,null,null,null,null,null,null,"Aug",186,593,186.49,181]
[null,null,null,null,null,null,null,null,null,null,"Sep",181,325,180.93,184]
[null,null,null,null,null,null,null,null,null,null,"Oct",173,303,172.59,181]
[null,null,null,null,null,null,null,null,null,null,"Nov",178,341,177.73,186]
[null,null,null,null,null,null,null,null,null,null,"Dec",176,262,176.05,187]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L22:L33)","v":179.09090909090909},{"$f":"MAX(M22:M33)","v":593},{"$f":"AVERAGE(N22:N33)","v":179.14636363636365},{"$f":"MAX(O22:O33)","v":190}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A3","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
["Comments :",null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L37:L48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M37:M48)","v":0},{"$f":"AVERAGE(N37:N48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O37:O48)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A4","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L52:L63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M52:M63)","v":0},{"$f":"AVERAGE(N52:N63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O52:O63)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A5","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L67:L78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M67:M78)","v":0},{"$f":"AVERAGE(N67:N78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O67:O78)","v":0}]

{"sheet":"TOC","index":18,"n_rows":79,"n_cols":17,"rows_kept":79,"cut":false,"hidden":false,"merged":[[3,16,7,18],[9,16,11,18],[12,16,15,18],[66,9,78,9],[4,1,4,3],[4,4,4,6],[4,9,4,14],[6,9,18,9],[21,9,33,9],[36,9,48,9],[47,0,47,6],[48,0,51,6],[51,9,63,9]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Monitoring of Total organic carbon emissions",null,null,"Whole Installation",null,null,"See  Notes in Cell Q3",null,null,{"$f":"+A3","v":"Monitoring of Total organic carbon emissions"},null,null,null,"Per Combustion Line",null,null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User to add logic to complete Whole installation, Table A5:G18. From the data in Per Combustion Line, Table J6:O79, subject to No. of lines installed"]
["mg/Nm3","1/2 Hourly Reference Periods",null,null,"Daily Reference Periods"]
[{"$f":"+'Cover Page'!C39","v":2023},"1/2 hourly TOC ELV","Monthly 1/2 hourly mean","Highest 1/2 hourly maximum","Daily TOC ELV","Monthly daily mean","Highest daily maximum",null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
["Jan",20,null,null,10,null,null,null,null,"A1","Jan"]
["Feb",20,1.5,9,10,1.44,2,null,null,null,"Feb",1,4,1.26,2]
["Mar",20,0.5,14,10,0.57999999999999996,2,null,null,null,"Mar",1,14,1.1000000000000001,2,null,"Whole Installation table A5:G18:"]
["Apr",20,1,39,10,0.81,1,null,null,null,"Apr",1,6,0.8,1,null,"Mean: for 1/2 hourly and daily periods calculate mean of values across all operational combustion lines for the month"]
["May",20,1,11,10,0.86,1,null,null,null,"May",1,6,0.83,1]
["Jun",20,1,41,10,0.81,1,null,null,null,"Jun",1,5,0.76,1]
["Jul",20,1,149,10,10.1,4,null,null,null,"Jul",1,149,0.93,4,null,"Maximum: for 1/2 hourly and daily periods use the highest value across all operational combustion lines for the month"]
["Aug",20,1.5,51,10,1.38,1,null,null,null,"Aug",1,9,0.91,1]
["Sep",20,0.5,16,10,-1.83,2,null,null,null,"Sep",1,16,0.97,2]
["Oct",20,1,13,10,1.03,1,null,null,null,"Oct",1,6,1,1]
["Nov",20,1,55,10,1.1000000000000001,5,null,null,null,"Nov",1,55,1.1299999999999999,5]
["Dec",20,1,186,10,1,5,null,null,null,"Dec",1,186,1.03,5]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L7:L18)","v":1},{"$f":"MAX(M7:M18)","v":186},{"$f":"AVERAGE(N7:N18)","v":0.97454545454545427},{"$f":"MAX(O7:O18)","v":5}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A2","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb",2,9,1.61,2]
[null,null,null,null,null,null,null,null,null,null,"Mar",0,7,0.06,2]
[null,null,null,null,null,null,null,null,null,null,"Apr",1,39,0.81,1]
[null,null,null,null,null,null,null,null,null,null,"May",1,11,0.88,1]
[null,null,null,null,null,null,null,null,null,null,"Jun",1,41,0.85,1]
[null,null,null,null,null,null,null,null,null,null,"Jul",1,7,1.08,3]
[null,null,null,null,null,null,null,null,null,null,"Aug",2,51,1.85,1]
[null,null,null,null,null,null,null,null,null,null,"Sep",0,12,-4.5599999999999996,1]
[null,null,null,null,null,null,null,null,null,null,"Oct",1,13,1.06,1]
[null,null,null,null,null,null,null,null,null,null,"Nov",1,6,1.06,2]
[null,null,null,null,null,null,null,null,null,null,"Dec",1,2,0.96,1]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L22:L33)","v":1},{"$f":"MAX(M22:M33)","v":51},{"$f":"AVERAGE(N22:N33)","v":0.51454545454545464},{"$f":"MAX(O22:O33)","v":3}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A3","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
["Comments :",null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L37:L48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M37:M48)","v":0},{"$f":"AVERAGE(N37:N48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O37:O48)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A4","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L52:L63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M52:M63)","v":0},{"$f":"AVERAGE(N52:N63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O52:O63)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A5","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L67:L78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M67:M78)","v":0},{"$f":"AVERAGE(N67:N78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O67:O78)","v":0}]

{"sheet":"Particulates","index":19,"n_rows":79,"n_cols":17,"rows_kept":79,"cut":false,"hidden":false,"merged":[[3,16,7,18],[9,16,11,18],[12,16,15,18],[66,9,78,9],[4,1,4,3],[4,4,4,6],[4,9,4,14],[6,9,18,9],[21,9,33,9],[36,9,48,9],[47,0,47,6],[48,0,51,6],[51,9,63,9]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Monitoring of Particulate matter emissions",null,null,"Whole Installation",null,null,"See  Notes in Cell Q3",null,null,{"$f":"+A3","v":"Monitoring of Particulate matter emissions"},null,null,null,"Per Combustion Line",null,null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User to add logic to complete Whole installation, Table A5:G18. From the data in Per Combustion Line, Table J6:O79, subject to No. of lines installed"]
["mg/Nm3","1/2 Hourly Reference Periods",null,null,"Daily Reference Periods"]
[{"$f":"+'Cover Page'!C39","v":2023},"1/2 hourly PM ELV","Monthly 1/2 hourly mean","Highest 1/2 hourly maximum","Daily PM ELV","Monthly daily mean","Highest daily maximum",null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
["Jan",30,null,null,10,null,null,null,null,"A1","Jan"]
["Feb",30,0.5,3,10,0.84,2,null,null,null,"Feb",0,2,0.33,0]
["Mar",30,0.5,2,10,0.68,1,null,null,null,"Mar",0,1,0.23,0,null,"Whole Installation table A5:G18:"]
["Apr",30,0.5,4,10,0.82,2,null,null,null,"Apr",0,2,0.28999999999999998,1,null,"Mean: for 1/2 hourly and daily periods calculate mean of values across all operational combustion lines for the month"]
["May",30,0.5,2,10,0.63,1,null,null,null,"May",0,1,0.25,0]
["Jun",30,0.5,3,10,0.69,2,null,null,null,"Jun",0,0,0.26,0]
["Jul",30,0.5,2,10,0.67,1,null,null,null,"Jul",0,1,0.25,0,null,"Maximum: for 1/2 hourly and daily periods use the highest value across all operational combustion lines for the month"]
["Aug",30,0.5,6,10,0.7,1,null,null,null,"Aug",0,2,0.27,0]
["Sep",30,1.5,31,10,1.39,3,null,null,null,"Sep",1,12,0.85,1]
["Oct",30,0.5,2,10,0.59,1,null,null,null,"Oct",0,2,0.49,1]
["Nov",30,1,24,10,0.75,3,null,null,null,"Nov",1,24,0.64,2]
["Dec",30,1,4,10,0.55000000000000004,1,null,null,null,"Dec",1,4,0.55000000000000004,1]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L7:L18)","v":0.27272727272727271},{"$f":"MAX(M7:M18)","v":24},{"$f":"AVERAGE(N7:N18)","v":0.40090909090909094},{"$f":"MAX(O7:O18)","v":2}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A2","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb",1,3,1.34,2]
[null,null,null,null,null,null,null,null,null,null,"Mar",1,2,1.1299999999999999,1]
[null,null,null,null,null,null,null,null,null,null,"Apr",1,4,1.35,2]
[null,null,null,null,null,null,null,null,null,null,"May",1,2,1.01,1]
[null,null,null,null,null,null,null,null,null,null,"Jun",1,3,1.1200000000000001,2]
[null,null,null,null,null,null,null,null,null,null,"Jul",1,2,1.08,1]
[null,null,null,null,null,null,null,null,null,null,"Aug",1,6,1.1200000000000001,1]
[null,null,null,null,null,null,null,null,null,null,"Sep",2,31,1.93,3]
[null,null,null,null,null,null,null,null,null,null,"Oct",1,1,0.69,1]
[null,null,null,null,null,null,null,null,null,null,"Nov",1,12,0.85,3]
[null,null,null,null,null,null,null,null,null,null,"Dec",1,2,0.55000000000000004,1]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L22:L33)","v":1.0909090909090908},{"$f":"MAX(M22:M33)","v":31},{"$f":"AVERAGE(N22:N33)","v":1.1063636363636364},{"$f":"MAX(O22:O33)","v":3}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A3","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
["Comments :",null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L37:L48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M37:M48)","v":0},{"$f":"AVERAGE(N37:N48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O37:O48)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A4","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L52:L63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M52:M63)","v":0},{"$f":"AVERAGE(N52:N63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O52:O63)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A5","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L67:L78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M67:M78)","v":0},{"$f":"AVERAGE(N67:N78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O67:O78)","v":0}]

{"sheet":"CO 95% 10 min","index":20,"n_rows":79,"n_cols":19,"rows_kept":79,"cut":false,"hidden":false,"merged":[[3,18,7,20],[9,18,11,20],[12,18,15,20],[66,10,78,10],[4,1,4,4],[4,5,4,7],[4,10,4,16],[6,10,18,10],[21,10,33,10],[36,10,48,10],[47,0,47,7],[48,0,51,7],[51,10,63,10]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Monitoring of Carbon Monoxide (10-minute avg)",null,null,null,"Whole Installation",null,null,"See  Notes in Cell S3",null,{"$f":"+A3","v":"Monitoring of Carbon Monoxide (10-minute avg)"},null,null,null,null,"Per Combustion Line",null,"Notes:",null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User to add logic to complete Whole installation, Table A5:H18. From the data in Per Combustion Line, Table K6:Q79, subject to No. of lines installed"]
["mg/Nm3","10-minute Reference Periods",null,null,null,"Daily Reference Periods"]
[{"$f":"+'Cover Page'!C39","v":2023},"95%ile 10-min avg CO ELV","95%ile 10-min avg maximum","Monthly CO 10-min avg mean","10-min avg maximum","Daily CO ELV","Monthly daily mean","Highest daily maximum",null,null,{"$f":"+A6","v":2023},"mg/Nm3","95%ile 10-min avg maximum","Monthly CO 10-min avg mean","10-min avg maximum","Monthly daily mean","Monthly daily maximum"]
["Jan",150,null,null,null,50,null,null,null,null,"A1","Jan"]
["Feb",{"$f":"+B7","v":150},16.77,8.5,35.5,{"$f":"+F7","v":50},8.56,17,null,null,null,"Feb",16.77,7,38,7.3,17]
["Mar",{"$f":"+B8","v":150},14.9,9.5,163.5,{"$f":"+F8","v":50},9.39,42,null,null,null,"Mar",12.31,7,84,7.02,26,null,"Whole Installation table A5:H18:"]
["Apr",150,12.46,8,26,50,7.93,15,null,null,null,"Apr",8.4,5,20,5.18,9,null,"Mean: for 10-min and daily periods use average of all operational combustion lines."]
["May",150,7.53,5.5,23.5,50,5.68,8,null,null,null,"May",6.61,5,22,4.96,7]
["Jun",150,8.3699999999999992,6,18.5,50,5.99,9,null,null,null,"Jun",7.58,5,24,4.91,9]
["Jul",150,11.73,6,20,50,5.99,33,null,null,null,"Jul",14.2,6,22,5.51,33,null,"Maximum: for 10-min and daily periods use the highest of all operational combustion lines in any month."]
["Aug",150,14.32,27.5,2030.5,50,32.04,13,null,null,null,"Aug",5.39,3,13,3.24,5]
["Sep",150,44.5,22,131.5,50,21.84,48,null,null,null,"Sep",30.42,16,97,16.5,35]
["Oct",150,23.1,13.5,115,50,13.66,37,null,null,null,"Oct",14.19,9,75,9.0299999999999994,14]
["Nov",150,70.45,19,952,50,18.3,176,null,null,null,"Nov",66.290000000000006,15,1385,15.43,176]
["Dec",150,16.09,10,61,50,10.02,30,null,null,null,"Dec",12.87,7,55,6.88,30]
[null,null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(M7:M18)","v":17.73},null,{"$f":"MAX(O7:O18)","v":1385},{"$f":"AVERAGE(P7:P18)","v":7.8145454545454553},{"$f":"MAX(Q7:Q18)","v":176}]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","95%ile 10-min avg maximum","Monthly CO 10-min avg mean","10-min avg maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,null,"A2","Jan"]
[null,null,null,null,null,null,null,null,null,null,null,"Feb",16.760000000000002,10,33,9.81,17]
[null,null,null,null,null,null,null,null,null,null,null,"Mar",17.489999999999998,12,243,11.76,42]
[null,null,null,null,null,null,null,null,null,null,null,"Apr",16.52,11,32,10.67,15]
[null,null,null,null,null,null,null,null,null,null,null,"May",8.44,6,25,6.39,8]
[null,null,null,null,null,null,null,null,null,null,null,"Jun",9.16,7,13,7.08,9]
[null,null,null,null,null,null,null,null,null,null,null,"Jul",9.25,6,18,6.46,12]
[null,null,null,null,null,null,null,null,null,null,null,"Aug",23.24,52,4048,60.84,13]
[null,null,null,null,null,null,null,null,null,null,null,"Sep",58.58,28,166,27.18,48]
[null,null,null,null,null,null,null,null,null,null,null,"Oct",31.92,18,155,18.29,37]
[null,null,null,null,null,null,null,null,null,null,null,"Nov",74.61,23,519,21.16,112]
[null,null,null,null,null,null,null,null,null,null,null,"Dec",19.309999999999999,13,67,13.15,21]
[null,null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(M22:M33)","v":25.934545454545457},null,{"$f":"MAX(O22:O33)","v":4048},{"$f":"AVERAGE(P22:P33)","v":17.526363636363637},{"$f":"MAX(Q22:Q33)","v":112}]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","95%ile 10-min avg maximum","Monthly CO 10-min avg mean","10-min avg maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,null,"A3","Jan"]
[null,null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,null,"Nov"]
["Comments :",null,null,null,null,null,null,null,null,null,null,"Dec"]
["Environment Agency explanatory note: The 10-minute average ELV is based on the “95th percentile”. In this case this means that 95% of the 10 minute averages in the relevant 24-hour period (i.e. 137) must be below 150 mg/Nm3, and 5% (i.e. 7) are allowed to be any value above 150 mg/Nm3. Whilst we expect operators to minimise CO emissions at all times, it is perfectly acceptable for the value of the maximum 10-minute average to be above 150 mg/Nm3, provided the 95th percentile ELV has been met for that period. ",null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(M37:M48)","v":{"$error":"#DIV/0!"}},null,{"$f":"MAX(O37:O48)","v":0},{"$f":"AVERAGE(P37:P48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(Q37:Q48)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","95%ile 10-min avg maximum","Monthly CO 10-min avg mean","10-min avg maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,null,"A4","Jan"]
[null,null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(M52:M63)","v":{"$error":"#DIV/0!"}},null,{"$f":"MAX(O52:O63)","v":0},{"$f":"AVERAGE(P52:P63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(Q52:Q63)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","95%ile 10-min avg maximum","Monthly CO 10-min avg mean","10-min avg maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,null,"A5","Jan"]
[null,null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(M67:M78)","v":{"$error":"#DIV/0!"}},null,{"$f":"MAX(O67:O78)","v":0},{"$f":"AVERAGE(P67:P78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(Q67:Q78)","v":0}]

{"sheet":"NH3","index":21,"n_rows":79,"n_cols":17,"rows_kept":79,"cut":false,"hidden":false,"merged":[[3,16,7,18],[9,16,11,18],[12,16,15,18],[66,9,78,9],[4,1,4,3],[4,4,4,6],[4,9,4,14],[6,9,18,9],[21,9,33,9],[36,9,48,9],[47,0,47,6],[48,0,51,6],[51,9,63,9]]}
[{"$f":"+'Cover Page'!$B$29","v":"Annual Performance Report 2023"},null,null,null,{"$f":"+'Cover Page'!$B$33","v":"Dudley Energy from Waste"}]
[]
["Monitoring of Ammnonia emissions ",null,null,"Whole Installation",null,null,"See  Notes in Cell Q3",null,null,{"$f":"+A3","v":"Monitoring of Ammnonia emissions "},null,null,null,"Per Combustion Line",null,null,"Notes:"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"User to add logic to complete Whole installation, Table A5:G18. From the data in Per Combustion Line, Table J6:O79, subject to No. of lines installed"]
["mg/Nm3","1/2 Hourly Reference Periods",null,null,"Daily Reference Periods"]
[{"$f":"+'Cover Page'!C39","v":2023},"1/2 hourly NH3 ELV","Monthly 1/2 hourly mean","Highest 1/2 hourly maximum","Daily NH3 ELV","Monthly daily mean","Highest daily maximum",null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
["Jan",0,null,null,10,null,null,null,null,"A1","Jan"]
["Feb",{"$f":"+B7","v":0},5,101,{"$f":"+E7","v":10},4.92,11,null,null,null,"Feb",6,37,6.05,11]
["Mar",{"$f":"+B8","v":0},6,91,{"$f":"+E8","v":10},6.22,10,null,null,null,"Mar",6,57,6.44,10,null,"Whole Installation table A5:G18:"]
["Apr",0,6.5,76,10,6.56,9,null,null,null,"Apr",6,16,6.45,8,null,"Mean: for 1/2 hourly and daily periods calculate mean of values across all operational combustion lines for the month"]
["May",0,6,23,10,5.98,8,null,null,null,"May",5,23,5.17,7]
["Jun",0,5.5,112,10,5.61,13,null,null,null,"Jun",4,25,4.08,7]
["Jul",0,6.5,434,10,6.27,16,null,null,null,"Jul",7,434,6.78,16,null,"Maximum: for 1/2 hourly and daily periods use the highest value across all operational combustion lines for the month"]
["Aug",0,11.5,1041,10,11.51,10,null,null,null,"Aug",4,8,3.96,4]
["Sep",0,19.5,148,10,19.73,54,null,null,null,"Sep",27,107,27.23,54]
["Oct",0,13.5,141,10,13.57,38,null,null,null,"Oct",15,141,15.37,38]
["Nov",0,13,279,10,12.86,48,null,null,null,"Nov",12,279,11.9,48]
["Dec",0,9,192,10,8.94,15,null,null,null,"Dec",9,192,8.5299999999999994,15]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L7:L18)","v":9.1818181818181817},{"$f":"MAX(M7:M18)","v":434},{"$f":"AVERAGE(N7:N18)","v":9.2690909090909095},{"$f":"MAX(O7:O18)","v":54}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A2","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb",4,101,3.78,8]
[null,null,null,null,null,null,null,null,null,null,"Mar",6,91,6,10]
[null,null,null,null,null,null,null,null,null,null,"Apr",7,76,6.66,9]
[null,null,null,null,null,null,null,null,null,null,"May",7,16,6.78,8]
[null,null,null,null,null,null,null,null,null,null,"Jun",7,112,7.13,13]
[null,null,null,null,null,null,null,null,null,null,"Jul",6,38,5.75,9]
[null,null,null,null,null,null,null,null,null,null,"Aug",19,1041,19.05,10]
[null,null,null,null,null,null,null,null,null,null,"Sep",12,148,12.22,25]
[null,null,null,null,null,null,null,null,null,null,"Oct",12,102,11.76,17]
[null,null,null,null,null,null,null,null,null,null,"Nov",14,182,13.81,31]
[null,null,null,null,null,null,null,null,null,null,"Dec",9,42,9.35,15]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L22:L33)","v":9.3636363636363633},{"$f":"MAX(M22:M33)","v":1041},{"$f":"AVERAGE(N22:N33)","v":9.2990909090909089},{"$f":"MAX(O22:O33)","v":31}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A3","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
["Comments :",null,null,null,null,null,null,null,null,null,"Dec"]
["An indicated ELV value of zero in the table above means that no ammonia limit is set in the permit.  ",null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L37:L48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M37:M48)","v":0},{"$f":"AVERAGE(N37:N48)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O37:O48)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A4","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L52:L63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M52:M63)","v":0},{"$f":"AVERAGE(N52:N63)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O52:O63)","v":0}]
[]
[null,null,null,null,null,null,null,null,null,{"$f":"+A6","v":2023},"mg/Nm3","Monthly 1/2 hourly mean","Monthly 1/2 hourly maximum","Monthly daily mean","Monthly daily maximum"]
[null,null,null,null,null,null,null,null,null,"A5","Jan"]
[null,null,null,null,null,null,null,null,null,null,"Feb"]
[null,null,null,null,null,null,null,null,null,null,"Mar"]
[null,null,null,null,null,null,null,null,null,null,"Apr"]
[null,null,null,null,null,null,null,null,null,null,"May"]
[null,null,null,null,null,null,null,null,null,null,"Jun"]
[null,null,null,null,null,null,null,null,null,null,"Jul"]
[null,null,null,null,null,null,null,null,null,null,"Aug"]
[null,null,null,null,null,null,null,null,null,null,"Sep"]
[null,null,null,null,null,null,null,null,null,null,"Oct"]
[null,null,null,null,null,null,null,null,null,null,"Nov"]
[null,null,null,null,null,null,null,null,null,null,"Dec"]
[null,null,null,null,null,null,null,null,null,null,"Annual",{"$f":"AVERAGE(L67:L78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(M67:M78)","v":0},{"$f":"AVERAGE(N67:N78)","v":{"$error":"#DIV/0!"}},{"$f":"MAX(O67:O78)","v":0}]